Design Rules

0.5 ¯m CMOS inverter

4005